543383

Design Floor
Description: DISANO by HARO Saphir Plank 1-Strip 4VM Light Oak brushed 543383
Design: Plank 1-Strip
Style: Light Oak
Surface: brushed
Bevel: 4VM
Installation system: Top Connect
Dimensions mm (HxWxL): 4,50 x 235,00 x 1282,00
PU (boards): 10 piece
PU (M2): 3,010 m²
Level of use (private/commercial): 23 / 33
Installation: Floating or glue-down installation
Made in Germany
Guarantee (private): 25
Blue Angel: yes
ECO Label: ID 0820-11848-007
CE label: yes
Ideal for underfloor heating: yes
Thermal resistance: 0,0317 m² K/W
Flammability class: CFLS2 / DFLS2
Slip resistance: R9
plasticizer-free
waterproof
Item number: 543383