543729

Design Floor
Description: DISANO by HARO ClassicAqua Plank 1-Strip XL 4V Crystal Oak brushed 543729
Design: Plank 1-Strip XL
Style: Crystal Oak
Surface: brushed
Bevel: 4V
Installation system: Top Connect
Dimensions mm (HxWxL): 9,80 x 235,00 x 2035,00
PU (boards): 5 piece
PU (M2): 2,390 m²
Level of use (private/commercial): 23 / 33
Installation: Floating or glue-down installation
Made in Germany
Guarantee (private): 25
Blue Angel: yes
ECO Label: ID 0820-11848-001
CE label: yes
Ideal for underfloor heating: yes
Thermal resistance: 0,063 m² K/W
Flammability class: CFLS1 / DFLS1
Slip resistance: R9
plasticizer-free
Suitable for installation in wet areas
Item number: 543729