544015

Design Floor
Description: DISANO by HARO WaveAqua Plank 1-Strip 4V Eiche Steady authentic 544015
Design: Plank 1-Strip
Style: Eiche Steady
Surface: authentic
Bevel: 4V
Installation system: Top Connect
Dimensions mm (HxWxL): 8,00 x 193,00 x 1282,00
PU (boards): 8 piece
PU (M2): 1,980 m²
Level of use (private/commercial): 23 / 33
Installation: Floating or glue-down installation
Made in Germany
Guarantee (private): 20
Blue Angel: yes
ECO Label: ID 0820-11848-009
CE label: yes
Ideal for underfloor heating: yes
Thermal resistance: 0,063 m² K/W
Flammability class: CFLS1
Slip resistance: R9
plasticizer-free
Suitable for installation in wet areas
Item number: 544015