530278

Laminate
Description: HARO Special Edition NKL31 Graphite Oak text. matt 530278
Style: Graphite Oak
Surface: text. matt
Installation system: Lock Connect plus
Dimensions mm (HxWxL): 7,00 x 193,00 x 1282,00
PU (boards): 9 piece
PU (M2): 2,220 m²
Level of use (private/commercial): 23 / 31
Abrasion resistance: AC3
Installation: Floating or glue-down installation
Made in Germany
Guarantee (private): 15
Blue Angel: yes
CE label: yes
Ideal for underfloor heating: yes
Thermal resistance: 0,058 m² K/W
Flammability class: CFLS1
Slip resistance: R9
Antistatic class Standard: DIN EN 1815
Impact resistance class: ≥ 8 N / ≥ 500 mm
plasticizer-free
Item number: 530278