532063

Laminate
Description: HARO TRITTY 100 Campus 4V Alpine Oak Nature authentic matt 532063
Design: Campus
Style: Alpine Oak Nature
Surface: authentic matt
Bevel: 4V
Installation system: Top Connect
Dimensions mm (HxWxL): 8,00 x 243,00 x 1282,00
PU (boards): 8 piece
PU (M2): 2,490 m²
Level of use (private/commercial): 23 / 32
Abrasion resistance: AC4
Installation: Floating or glue-down installation
Made in Germany
Guarantee (private): 25
Blue Angel: yes
CE label: yes
Ideal for underfloor heating: yes
Thermal resistance: 0,065 m² K/W
Flammability class: CFLS1
Slip resistance: R9
Antistatic class Standard: DIN EN 1815
Impact resistance class: ≥ 12 N / ≥ 750 mm
plasticizer-free
Item number: 532063