539089

Parquet
Description: HARO 4000 Plank 1-Strip 180 4V Oak Reed Brown Sauvage brushed naturaLin plus 539089
Design: Plank 1-Strip 180
Type of wood: Oak Reed Brown
Grade: Sauvage
Surface: brushed naturaLin plus
Bevel: 4V
Installation system: Top Connect
Dimensions mm (HxWxL): 13,50 x 180,00 x 2200,00
Top layer: ca. 3,5 mm
PU (boards): 8 piece
PU (M2): 3,170 m²
Technical construction: 3-layer / Solid fingerstrips as middle layer
Installation: Floating or glue-down installation
Made in Germany
Guarantee (private): 30
Blue Angel: yes
CE label: yes
Ideal for underfloor heating: yes
Thermal resistance: 0,110 m² K/W
Flammability class: CFLS1
Slip resistance: R10
Chair caster resistance: DIN EN 425
HARO Parquet 70% PEFC-certified
plasticizer-free
Item number: 539089